**Atmospheric Correction Tool for WISE MAN (ACWISE)**

**User Manual (v0.1)**

Yanqun Pan, 2020/09/24

**Introduction**

**ACWISE** is a software package which is developed for atmospheric correction of WISE image. For the current version (v0.1), it can only handle the Level1G images which are geo-referenced radiance. To run it successfully, some other WISE data are also needed, like the navigation log and geo reference LUTs, etc. More details are given in section 4.

This package was written in pure Python, it runs in environment of Python>=3.5, but it may occur some warnings in Python 3.7 and 3.8. To run it, a bunch of 3rd part of libraries are required. To make it easier for user who is not very familiar with Python, this package is installed in a singularity image and all of the dependencies have been installed.

**Quick start**

Following the steps below to run it:


1. Go into the singularity sif image. Note that users don’t have the write permission, so it needs to mount the external directory that contains the WISE images to be processed.

singularity shell --bind /data:/mnt acwise.sif


1. Set the run environment



1. Run acwise to get help info




1. To run acwise, a configure file is mandatory.



**The configure file**

To make the software package more extensible, a bunch of options can be set in the configure file. But for the current version which only implemented the basic function, most of options are fixed. Here is a template for the configure file, the options marked as yellow are fixed, it can not be modified by now. The details of the options are given as below:



**[WISE]**

This is set for the input of the level-1 WISE image. **IMAGE\_NAME** refers to the name of the image to be processed, for the pattern of the image name, please refers to the WISE flight document. L1G\_DIR is for the directory that contains the L1G images. L1A\_GLU\_DIR and NAV\_LOG\_DIR are for the directories that contain the geo-reference LUTs ($IMAGE\_NAME$-L1A.glu.hdr) and the navigation log files ($IMAGE\_NAME$-Navcor\_sum.log), respectively.

**[AC]**

This section configures some general information about atmospheric correction. Currently, the entire image will be split into several tiles (squares) for processing. The **TILE\_SIZE** option is for the size of each tile, the unit of the size is *km.* **PROCEDURE= STANDADRD** means the atmospheric correction will be performed in a standard procedure, step by step. Except for STANDARD, the other kinds of procedure is not implemented yet. The **STANDARD** procedure is further configured in the **STANDARD** section. The ancillary data mainly includes the total concentration of **OZONE** (m.atm)**,WATER VAPOR** (g cm2) and **WIND SPEED** (m s-1). These data can only be fixed manually, since the automatically way is not implemented yet.

**[STANDARD]**

This section is set for the gas absorption, Rayleigh, glint, adjacency effect and aerosol correction. Note that adjacency effect correction algorithm was not implemented yet, so the option of **ADJ\_ALGORIHTM** should be set **None**. The calculation of gas absorption, Rayleigh and aerosol are all based on 6SV, so they are set as **SixS**. The calculation of glint is based on the Cox&Munk model, so **GLINT\_CALCULATION=CoxMunk**. For the aerosol retrieval algorithm, only the **DSF** (Quinten et al,2018) algorithm is implemented in current version, so **AERO\_ALGORIHTM=DSF** (the details of DSF is further configured in the DSF section). If one of the options are set **None**, the related correction will be skipped, for example, no aerosol correction will be performed when **AERO\_ALGORIHTM** **=None**, but the Rayleigh correction is mandatory, mean **RAY\_CALCULATOR** should not be set **None**.

**[DSF]**

The darkest pixel could be determined directly or by linear fitting, which is controlled by the **FITTING** option, the value of 1 and 0 is a switch of using linear fitting or not. **DARK\_SPECTRUM\_NUM** determines the number of bands of the darkest pixel. For the hyperspectral WISE image, the default value is set 5, which means the aerosol reflectance spectra will be determined by darkest pixels in 5 bands. **DARK\_PIXEL\_NUM** is the number (the default value is 20) of real darkest pixels which are used to determine the ideal darkest pixel by linear fitting, it works only when **FITTING=1**.

**[OUTPUT]**

The level-2 file is save as GEOTIFF. Currently, only the Rrs product is saved in the level-2 file. The DIR option specifies the directory to save the level-2 file, and NAME specifies the name of the level-2 file. **$NAME$** will be replaced by **IMAGE\_NAME**.

**[DATA]**

DATA\_DIR specifies the directory that contains the internal data that will be used by the package. By default, the data will be located in **/opt/acwise\_data**.